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Section 092216 Non-Structural Metal Framing
NOTE:
Turn on hidden text to view important non-printing notes by selecting Show/Hide (¶) in the Paragraph Group, or by using the Ctrl+* keyboard shortcut.
PART 1 -  GENERAL
1.1 QUALITY ASSURANCE
A. [bookmark: _Hlk172123123][bookmark: _Hlk156891605][bookmark: _Hlk172122996][bookmark: _Hlk188511479]Code-Compliance Certification of Studs and Tracks: Provide documentation that framing members are certified in accordance with the product-certification program of the Steel Framing Industry Association (SFIA) or similar organization providing a verifiable code-compliance program.
PART 2 -  PRODUCTS
2.1 NON-STRUCTURAL METAL FRAMING
[bookmark: _Hlk175904230][bookmark: _Hlk196817146][bookmark: _Hlk161393966][bookmark: _Hlk169529121]Retain first option in "Framing Members, General" Paragraph below for 2015 IBC; second option for 2018 IBC, 2021 IBC, or 2024 IBC.
A. [bookmark: _Hlk186200377][bookmark: _Hlk165966591]Framing Members, General: Comply with [AISI S220 and ASTM C645, Section 10] [AISI S220] for conditions indicated.
1. [bookmark: _Hlk173308857][bookmark: _Hlk159399184][bookmark: _Hlk188522475][bookmark: _Hlk210396894][bookmark: _Hlk173308975][bookmark: _Hlk159399243]Protective Coating: [Coating with equivalent corrosion resistance of ASTM A653/A653M, G40 (Z120)] [ASTM A653/A653M, G40 (Z120)] [ASTM A653/A653M, G60 (Z180)] [ASTM A653/A653M, G90 (Z275)] unless otherwise indicated. Galvannealed products are not acceptable.
B. [bookmark: _Hlk160704452][bookmark: _Hlk159505061]Slip-Type Head Joints: Where indicated, provide[ one of] the following:
Retain “Head-of-Wall Sound Isolation Clip System” if required. In full height walls, the ClarkDietrich ProSTUD Motion Frame Connector is installed at the top of each metal stud to mitigate sound caused by vertical and lateral movement of tall buildings. Instead of utilizing traditional top track types, the ProSTUD Motion Frame Connector is nested between horizontal ProSTUD members that are attached overhead to the concrete floor assembly.
The Motion Frame Dynamic Head-of-Wall System is tested with 2-1/2- and 3-5/8-inch (64- and 92-mm) ProSTUD depths for both new and retrofit construction in accordance with UL2079, for use in specified 1-hour Fire-Resistive Joint Systems, 2-hour Fire-Resistive Joint Systems and 2-hour Nonbearing Wall Assemblies.
1. Head-of-Wall Sound Isolation Clip System: Fabricated from fire-resistant, ABS polymer; eliminates metal-to-metal contact at head-of-wall connection while accommodating vertical and lateral movement. Tested system consists of horizontal and vertical proprietary stud members.
a. Product: ClarkDietrich; ProSTUD Drywall Framing System and Motion Frame™ Connector.
1) Minimum Base-Steel Thickness: [As indicated on Drawings] [As required by performance requirements for horizontal deflection] [0.0150 inch (0.3810 mm)] [0.0181 inch (0.4597 mm)] [0.0296 inch (0.752 mm)] [0.0329 inch (0.836 mm)].
2) Flange Size: 1-1/4 inches (32 mm).
3) Web Depth: [2-1/2 inches (64 mm)] [3-5/8 inches (92 mm)].
4) Connector Depth: Matching stud web depth.
PART 3 -  EXECUTION
3.1 INSTALLATION, GENERAL
A. [bookmark: _Hlk161397347]Install Non-Structural Metal Framing Systems in accordance with ASTM C754 and manufacturer’s written instructions.
1. Install fire-rated partitions in compliance with requirements of UL assembly as indicated on drawings.
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